{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["【标表1】投标报价汇总表_(2009范本)","【标表2】工程量清单表"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":2,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"【标表1】投标报价汇总表_(2009范本)","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,0,0,5],[1,1,1,5],[2,1,2,3],[3,3,3,4],[4,3,4,4],[5,3,5,4],[6,3,6,4],[7,3,7,4],[8,3,8,4],[9,2,9,4],[10,2,10,4],[11,2,11,4],[12,2,12,4],[13,1,13,4],[1,0,11,0]],"flags":["formulas_cached_only"]}
[]
[null,"投标报价汇总表"]
[null,"合同段：1",null,null,"","标表1"]
[null,"序号","章次","科目名称",null,"金额（元）"]
[null,"1","100","    总    则",null,0]
[null,"2","200","    路    基",null,0]
[null,"3","300","    路    面",null,0]
[null,"3","400","    桥梁、涵洞",null,0]
[null,"4","600","    安全设施及预埋管线",null,0]
[null,"5","第100章至第700章合计",null,null,0]
[null,"6","暂列金额（不含计日工总额）"]
[null,"7","投标报价",null,null,0]
[null,"","",null,null,""]
[null,"清单   第 1 页",null,null,null,"共 1 页"]

{"sheet":"【标表2】工程量清单表","index":1,"n_rows":230,"n_cols":7,"rows_kept":230,"cut":false,"hidden":false,"merged":[[1,1,1,6],[2,1,2,2],[2,3,2,5],[3,1,3,6],[17,1,17,4],[18,1,18,5],[21,1,21,6],[22,1,22,2],[22,3,22,5],[23,1,23,6],[44,1,44,4],[45,1,45,5],[48,1,48,6],[49,1,49,2],[49,3,49,5],[50,1,50,6],[72,1,72,4],[73,1,73,5],[76,1,76,6],[77,1,77,2],[77,3,77,5],[78,1,78,6],[92,1,92,4],[93,1,93,5],[96,1,96,6],[97,1,97,2],[97,3,97,5],[98,1,98,6],[115,1,115,4],[116,1,116,5],[119,1,119,6],[120,1,120,2],[120,3,120,5],[121,1,121,6],[137,1,137,4],[138,1,138,5],[141,1,141,6],[142,1,142,2],[142,3,142,5],[143,1,143,6],[155,1,155,4],[156,1,156,5],[158,1,158,6],[159,1,159,2],[159,3,159,5],[160,1,160,6],[176,1,176,4],[177,1,177,5],[182,1,182,6],[183,1,183,2],[183,3,183,5],[184,1,184,6],[228,1,228,4],[229,1,229,5]],"flags":["formulas_cached_only"]}
[]
[null,"工程量清单表"]
[null,"合同段：1",null,"",null,null,"标表2"]
[null,"第100章    总    则"]
[null,"子目号","子目名称","单位","数量","单价","合价"]
[null,"101-1","保险费",""]
[null,"-a","按合同条款规定，提供建筑工程一切险","总额",null,null,0]
[null,"-b","按合同条款规定，提供第三者责任险","总额",null,null,0]
[null,"102-3","安全生产费","总额","1.000",null,0]
{"$rows_empty":7}
[null,"","","","","",""]
[null,"第100章  合计   人民币",null,null,null,0,"元"]
[null,"清单   第 1 页",{"$nulls":4},"共 9 页"]
[]
[]
[null,"工程量清单表"]
[null,"合同段：滑县X008焦虎至牛屯公路改建工程",null,"",null,null,"标表2"]
[null,"第200章    路    基"]
[null,"子目号","子目名称","单位","数量","单价","合价"]
[null,"202-2","挖除旧路面","","","",""]
[null,"-b","沥青混凝土路面","m3","425.000",null,0]
[null,"-d","水泥稳定碎石基层","m2",9010,null,0]
[null,"-e","石灰土底基层","m2","9520.000",null,0]
[null,"203-1","路基挖方","",""]
[null,"-a","挖土方","m3","11348.330",null,0]
[null,"-d","弃方"]
[null,"-d-1","弃土方","m3","4424.300",null,0]
[null,"204-1","路基填筑（包括填前压实）","",""]
[null,"-b","利用土方","m3","5968.920",null,0]
[null,"207-1","M7.5砂浆砖砌边沟"]
[null,"-a","M7.5砂浆砖砌边沟","m3","1252.500",null,0]
[null,"-c","C25盖板混凝土","m3","258.015",null,0]
[null,"-d","盖板钢筋","",""]
[null,"-d-1","光圆钢筋(R235)","kg","16783.500",null,0]
[null,"-d-2","带肋钢筋(HRB335、HRB400)","kg","13326.600",null,0]
[null,"-e","C20现浇混凝土","m3","240.480",null,0]
[null,"-f","M10砂浆抹面","m2","3757.500",null,0]
[null,"","","","","",""]
[null,"第200章  合计   人民币",null,null,null,0,"元"]
[null,"清单   第 2 页",{"$nulls":4},"共 9 页"]
[]
[]
[null,"工程量清单表"]
[null,"合同段：滑县X008焦虎至牛屯公路改建工程",null,"",null,null,"标表2"]
[null,"第300章    路    面"]
[null,"子目号","子目名称","单位","数量","单价","合价"]
[null,"304-3","水泥稳定土基层","","","",""]
[null,"-b","厚180mm"]
[null,"-b-3","碎石(水泥剂量5%)","m2","8900.000",null,0]
[null,"304-3","水泥稳定土基层","",""]
[null,"-b","厚180mm",null,""]
[null,"-b-3","碎石(水泥剂量5%)","m2","105870.000",null,0]
[null,"305-5","水泥石灰稳定底基层","",""]
[null,"-b","厚180mm"]
[null,"-b-1","土(4:10:86)","m2","9410.000",null,0]
[null,"308-1","透层","m2","105870.000",null,0]
[null,"308-2","黏层","m2",102480,null,0]
[null,"309-1","细粒式沥青混凝土","",""]
[null,"-a","厚250mm","m2","103533.760",null,0]
[null,"309-2","中粒式沥青混凝土","",""]
[null,"-a","厚450mm","m2","103533.760",null,0]
[null,"310-2","封层"]
[null,"-a","层铺法沥青表处封层","m2","105870.000",null,0]
[null,"313-1","培土路肩","",""]
[null,"-a","培土","m3","4502.520",null,0]
[null,"","","","","",""]
[null,"第300章  合计   人民币",null,null,null,0,"元"]
[null,"清单   第 3 页",{"$nulls":4},"共 9 页"]
[]
[]
[null,"工程量清单表"]
[null,"合同段：滑县X008焦虎至牛屯公路改建工程",null,"",null,null,"标表2"]
[null,"第600章    安全设施及预埋管线"]
[null,"子目号","子目名称","单位","数量","单价","合价"]
[null,"604-5","单悬臂式交通标志",null,"","",""]
[null,"-a","L=0.7m","个","10.000",null,0]
[null,"-b","D=0.6m","个","10.000",null,0]
[null,"-c","1.11m×0.72m","个","4.000",null,0]
[null,"-d","1.44m×0.72m","个","3.000",null,0]
[null,"604-8","里程碑","个","11.000",null,0]
[null,"604-9","公路界碑","个","57.000",null,0]
[null,"604-10","百米桩","个","113.000",null,0]
[null,"605-1","热熔型涂料路面标线","",""]
[null,"-a","热熔型涂料路面标线","m2","4068.000",null,0]
[null,"604-12","示警桩","个",22,null,0]
[null,"","","",""]
[null,"第600章  合计   人民币",null,null,null,0,"元"]
[null,"清单   第 4 页",{"$nulls":4},"共 9 页"]
[]
[]
[null,"工程量清单表"]
[null,"合同段：滑县X008牛屯至延津县界公路改建工程",{"$nulls":4},"标表2"]
[null,"第200章    路    基"]
[null,"子目号","子目名称","单位","数量","单价","合价"]
[null,"203-1","路基挖方"]
[null,"-a","挖土方","m3","1830.100",null,0]
[null,"-d","弃方"]
[null,"-d-1","弃土方","m3","1021.930",null,0]
[null,"204-1","路基填筑（包括填前压实）"]
[null,"-b","利用土方","m3","696.700",null,0]
[null,"207-1","M7.5砂浆砖砌边沟"]
[null,"-a","M7.5砂浆砖砌边沟","m3","150.000",null,0]
[null,"-c","C25盖板混凝土","m3","30.900",null,0]
[null,"-d","盖板钢筋"]
[null,"-d-1","光圆钢筋(R235)","kg","2010.000",null,0]
[null,"-d-2","带肋钢筋(HRB335、HRB400)","kg","1596.000",null,0]
[null,"-e","C20现浇混凝土","m3","28.800",null,0]
[null,"-f","M10砂浆抹面","m2","450.000",null,0]
[]
[null,"第200章  合计   人民币",null,null,null,0,"元"]
[null,"清单   第 5 页",{"$nulls":4},"共 9 页"]
[]
[]
[null,"工程量清单表"]
[null,"合同段：滑县X008牛屯至延津县界公路改建工程",{"$nulls":4},"标表2"]
[null,"第300章    路    面"]
[null,"子目号","子目名称","单位","数量","单价","合价"]
[null,"304-3","水泥稳定土基层"]
[null,"-b","厚180mm"]
[null,"-b-3","碎石(水泥剂量5%)","m2","26590.000",null,0]
[null,"308-1","透层","m2","26590.000",null,0]
[null,"308-2","黏层","m2",23730,null,0]
[null,"309-1","细粒式沥青混凝土"]
[null,"-a","厚250mm","m2","24578.770",null,0]
[null,"309-2","中粒式沥青混凝土"]
[null,"-a","厚450mm","m2","24578.770",null,0]
[null,"310-2","封层"]
[null,"-a","层铺法沥青表处封层","m2",26590,null,0]
[null,"313-1","培土路肩"]
[null,"-a","培土","m3","894.125",null,0]
[]
[null,"第300章  合计   人民币",null,null,null,0,"元"]
[null,"清单   第 6 页",{"$nulls":4},"共 9 页"]
[]
[]
[null,"工程量清单表"]
[null,"合同段：滑县X008牛屯至延津县界公路改建工程",{"$nulls":4},"标表2"]
[null,"第600章    安全设施及预埋管线"]
[null,"子目号","子目名称","单位","数量","单价","合价"]
[null,"604-5","单悬臂式交通标志"]
[null,"-a","L=0.7m","个","2.000",null,0]
[null,"-b","D=0.6m","个","4.000",null,0]
[null,"-c","1.44m×0.72m","个","2.000",null,0]
[null,"604-8","里程碑","个","2.000",null,0]
[null,"604-9","公路界碑","个","12.000",null,0]
[null,"604-10","百米桩","个","25.000",null,0]
[null,"605-1","热熔型涂料路面标线"]
[null,"-a","热熔型涂料路面标线","m2","891.000",null,0]
[]
[null,"第600章  合计   人民币",null,null,null,0,"元"]
[null,"清单   第 7 页",{"$nulls":4},"共 9 页"]
[]
[null,"工程量清单表"]
[null,"合同段：滑县引黄入内总干渠桥新建工程",{"$nulls":4},"标表2"]
[null,"第200章    路    基"]
[null,"子目号","子目名称","单位","数量","单价","合价"]
[null,"204-1","路基填筑（包括填前压实）"]
[null,"-g","结构物台背回填"]
[null,"-g-1","回填砂砾","m3",99.8,null,0]
{"$rows_empty":11}
[null,"第200章  合计   人民币",null,null,null,0,"元"]
[null,"清单   第 8 页",{"$nulls":4},"共 9 页"]
[]
[]
[]
[]
[null,"工程量清单表"]
[null,"合同段：滑县引黄入内总干渠桥新建工程",{"$nulls":4},"标表2"]
[null,"第400章    桥梁、涵洞"]
[null,"子目号","子目名称","单位","数量","单价","合价"]
[null,"403-1","基础钢筋(包括灌注桩、承台、沉桩、沉井等)"]
[null,"-a","光圆钢筋（HPB235、HPB300）","kg","846.800",null,0]
[null,"-b","带肋钢筋（HRB335、HRB400）","kg","5789.000",null,0]
[null,"403-2","下部结构钢筋"]
[null,"-a","光圆钢筋（HPB235、HPB300）","kg","781.900",null,0]
[null,"-b","带肋钢筋（HRB335、HRB400）","kg","2200.700",null,0]
[null,"403-3","上部结构钢筋"]
[null,"-a","光圆钢筋（HPB235、HPB300）","kg","1034.300",null,0]
[null,"-b","带肋钢筋（HRB335、HRB400）","kg","8396.900",null,0]
[null,"403-4","附属结构钢筋"]
[null,"-a","光圆钢筋（HPB235、HPB300）","kg","135.800",null,0]
[null,"-b","带肋钢筋(HRB335、HRB400)","kg","5257.400",null,0]
[null,"404-1","干处挖土方","m3","215.800",null,0]
[null,"405-1","钻孔灌注桩（φ1.5m）"]
[null,"-c","桩径1.5m","m","60.000",null,0]
[null,"410-2","混凝土下部结构"]
[null,"-a","轻型桥台(按混凝土等级分列)"]
[null,"-a-2","C25","m3","106.000",null,0]
[null,"-i","混凝土盖梁及耳背墙(按混凝土等级分列)"]
[null,"-i-2","C30","m3","32.200",null,0]
[null,"410-6","现浇混凝土附属结构"]
[null,"-c","护栏(按混凝土等级分列)"]
[null,"-c-1","C30","m3","19.000",null,0]
[null,"-d","桥头搭板(按混凝土等级分列)"]
[null,"-d-1","C30","m3","14.400",null,0]
[null,"-e","防震挡块"]
[null,"-e-2","C30","m3","0.300",null,0]
[null,"-f","支座垫石(按混凝土等级分列)"]
[null,"-f-1","C30","m3","0.200",null,0]
[null,"411-2","先张法预应力钢绞线","kg","1701.200",null,0]
[null,"411-7","现浇预应力混凝土上部结构"]
[null,"-d","混凝土铰缝、企口缝(按混凝土等级分列)"]
[null,"-d-1","C50","m3","8.800",null,0]
[null,"411-8","预制预应力混凝土上部结构"]
[null,"-c","空心板(按混凝土等级分列)"]
[null,"-c-3","C50","m3","49.500",null,0]
[null,"415-2","水泥混凝土桥面铺装(C40,厚120mm)"]
[null,"-b","C40防水混凝土厚120 mm","m2","100.000",null,0]
[null,"416-2","圆形板式橡胶支座"]
[null,"k","GYZF4200×30","个","20.000",null,0]
[null,"417-1","橡胶伸缩装置","m","9.600",null,0]
[]
[null,"第400章  合计   人民币",null,null,null,0,"元"]
[null,"清单   第 9 页",{"$nulls":4},"共 9 页"]